
Lab – Troubleshooting Inter-VLAN Routing

1. Topology



1. Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| R1 | G0/1.1 | 192.168.1.1 | 255.255.255.0 | N/A |
|  | G0/1.10 | 192.168.10.1 | 255.255.255.0 | N/A |
|  | G0/1.20 | 192.168.20.1 | 255.255.255.0 | N/A |
|  | Lo0 | 209.165.200.225 | 255.255.255.224 | N/A |
| S1 | VLAN 1 | 192.168.1.11 | 255.255.255.0 | 192.168.1.1 |
| S2 | VLAN 1 | 192.168.1.12 | 255.255.255.0 | 192.168.1.1 |
| PC-A | NIC | 192.168.10.3 | 255.255.255.0 | 192.168.10.1 |
| PC-B | NIC | 192.168.20.3 | 255.255.255.0 | 192.168.20.1 |

Switch Port Assignment Specifications

|  |  |  |
| --- | --- | --- |
| Ports | Assignment | Network |
| S1 F0/1 | 802.1Q Trunk | N/A |
| S2 F0/1 | 802.1Q Trunk | N/A |
| S1 F0/5 | 802.1Q Trunk | N/A |
| S1 F0/6 | VLAN 10 – R&D | 192.168.10.0/24 |
| S2 F0/18 | VLAN 20 – Engineering | 192.168.20.0/24 |

Objectives

Part 1: Build the Network and Load Device Configurations

Part 2: Troubleshoot the Inter-VLAN Routing Configuration

Part 3: Verify VLAN Configuration, Port Assignment, and Trunking

Part 4: Test Layer 3 Connectivity

1. Background / Scenario

The network has been designed and configured to support three VLANs. Inter-VLAN routing is provided by an external router using an 802.1Q trunk, also known as router-on-a-stick. Routing to a remote web server, which is simulated by Lo0, is also provided by R1. However, it is not working as designed, and user complaints have not given much insight into the source of the problems.

In this lab, you must first define what is not working as expected, and then analyze the existing configurations to determine and correct the source of the problems. This lab is complete when you can demonstrate IP connectivity between each of the user VLANs and the external web server network, and between the switch management VLAN and the web server network.

**Note**: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.

**Note**: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.

1. Required Resources

* 1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
* 2 Switches (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
* 2 PCs (Windows 7, Vista, or XP with terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

1. Build the Network and Load Device Configurations

In Part 1, you will set up the network topology and configure basic settings on the PC hosts, switches, and router.

* 1. Cable the network as shown in the topology.
  2. Configure PC hosts.

Refer to the Addressing Table for PC host address information.

* 1. Load router and switch configurations.

Load the following configurations into the appropriate router or switch. All devices have the same passwords; the enable password is **class**, and the line password is **cisco**.

Router R1 Configuration:

hostname R1

enable secret class

no ip domain lookup

line con 0

password cisco

login

logging synchronous

line vty 0 4

password cisco

login

interface loopback0

ip address 209.165.200.225 255.255.255.224

interface gigabitEthernet0/1

no ip address

interface gigabitEthernet0/1.1

encapsulation dot1q 11

ip address 192.168.1.1 255.255.255.0

interface gigabitEthernet0/1.10

encapsulation dot1q 10

ip address 192.168.11.1 255.255.255.0

interface gigabitEthernet0/1.20

encapsulation dot1q 20

ip address 192.168.20.1 255.255.255.0

end

Switch S1 Configuration:

hostname S1

enable secret class

no ip domain-lookup

line con 0

password cisco

login

logging synchronous

line vty 0 15

password cisco

login

vlan 10

name R&D

exit

interface fastethernet0/1

switchport mode access

interface fastethernet0/5

switchport mode trunk

interface vlan1

ip address 192.168.1.11 255.255.255.0

ip default-gateway 192.168.1.1

end

Switch S2 Configuration:

hostname S2

enable secret class

no ip domain-lookup

line con 0

password cisco

login

logging synchronous

line vty 0 15

password cisco

login

vlan 20

name Engineering

exit

interface fastethernet0/1

switchport mode trunk

interface fastethernet0/18

switchport access vlan 10

switchport mode access

interface vlan1

ip address 192.168.1.12 255.255.255.0

ip default-gateway 192.168.1.1

end

* 1. Save the running configuration to the startup configuration.

1. Troubleshoot the Inter-VLAN Routing Configuration

In Part 2, you will verify the inter-VLAN routing configuration.

1. On R1, enter the **show ip route** command to view the routing table.

Which networks are listed? \_\_\_\_\_\_209.165.200.224\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Are there any networks missing in the routing table? If so, which networks?

\_\_\_\_\_\_192.168.1.0, 192.168.10.0, 192.168.20.0\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

What is one possible reason that a route would be missing from the routing table?

\_\_\_\_\_\_Wyłączony interfejs albo brak zdefiniowanego adresu ip interfejsu \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. On R1, issue the **show ip interface brief** command.

Based on the output, are there any interface issues on the router? If so, what commands would resolve the issues?

\_\_\_int g0/1 → no shut → int g0/1.10 → ip address 192.168.10.1 255.255.255.0\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. On R1, re-issue the **show ip route** command.

Verify that all networks are available in the routing table. If not, continue to troubleshoot until all networks are present.

1. Verify VLAN Configuration, Port Assignment, and Trunking

In Part 3, you will verify that the correct VLANs exist on both S1 and S2 and that trunking is configured correctly.

* 1. Verify VLAN configuration and port assignments.
     1. On S1, enter the **show vlan brief** command to view the VLAN database.

Which VLANs are listed? Ignore VLANs 1002 to 1005.

\_\_VLAN 1, VLAN 10\_\_\_\_\_

Are there any VLANs numbers or names missing in the output? If so, list them.

\_\_\_\_\_VLAN 20 Engineering\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Are the access ports assigned to the correct VLANs? If not, list the missing or incorrect assignments.

\_\_\_int fa0/6 musi zostać przypisany do vlan 10 \_\_\_

If required, what commands would resolve the VLAN issues?

vlan 20 → name Engineering → exit → int fa0/6 → switchport mode access → switchport access vlan 10 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. On S1, re-issue the **show vlan brief** command to verify configuration.
    2. On S2, enter the **show vlan brief** command to view the VLAN database.

Which VLANs are listed? Ignore VLANs 1002 to 1005.

\_\_\_\_\_\_VLAN 1, VLAN 10, VLAN 20\_\_\_\_\_\_\_

Are there any VLANs numbers or names missing in the output? If so, list them.

\_\_\_\_\_VLAN 10 brakuje mu nazwy R&D ale nie usimy jej nadawać ponieważ S2 ma widzieć VLAN 1 I VLAN 20 \_\_\_\_\_\_\_

Are the access ports assigned to the correct VLANs? If not, list the missing or incorrect assignments.

\_\_\_\_int fa0/18 powinien być przypisany do vlan 20 zamiast vlan 10\_\_\_\_\_\_\_\_\_\_

If required, what commands would resolve the VLAN issues?

\_\_int fa0/18 → switchport access vlan 20 → exit → int vlan 1 → no shut → end → conf t → no vlan 10 → exit \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. On S2, re-issue the **show vlan brief** command to verify any configuration changes.
  1. Verify trunking interfaces.
     1. On S1, enter the **show interface trunk** command to view the trunking interfaces.

Which ports are in trunking mode? \_\_\_fa0/5\_\_\_\_

Are there any ports missing in the output? If so, list them. \_\_\_fa0/1\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

If required, what commands would resolve the port trunking issues?

\_\_\_int fa0/1 → switchport mode trunk\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. On S1, re-issue the **show interface trunk** command to verify any configuration changes.
    2. On S2, enter the **show interface trunk** command to view the trunking interfaces.

Which ports are in trunking mode? \_\_fa0/1\_\_

Are there any ports missing in the output? If so, list them. \_\_\_\_\_\_nie brakuje\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

If required, what commands would resolve the port trunking issues?

\_\_wszystkie porty są skonfigurowane poprawnie \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Test Layer 3 Connectivity
2. Now that you have corrected multiple configuration issues, let’s test connectivity.

From PC-A, is it possible to ping the default gateway for VLAN 10? \_\_\_tak\_\_\_\_\_

From PC-A, is it possible to ping PC-B? \_\_tak\_\_\_\_\_\_\_

From PC-A, is it possible to ping Lo0? \_\_\_tak\_\_\_\_

If the answer is **no** to any of these questions, troubleshoot the configurations and correct the error.

**Note**: It may be necessary to disable the PC firewall for pings between PCs to be successful.

From PC-A, is it possible to ping S1? \_\_\_\_nie\_\_\_\_\_

From PC-A, is it possible to ping S2? \_\_\_\_\_nie\_\_\_

List some of the issues that could still be preventing successful pings to the switches.

\_\_\_\_niepoprawne przypisanie sieci vlan na interface routera, niepoprawny adres IP na switchu brak bramy na switchu\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. One way to help resolve where the error is occurring is to do a **tracert** from PC-A to S1.

C:\Users\User1> **tracert 192.168.1.11**

Tracing route to 192.168.1.11 over a maximum of 30 hops

1 <1 ms <1 ms <1 ms 192.168.10.1

2 \* \* \* Request timed out.

3 \* \* \* Request timed out.

<output omitted>

This output shows that the request from PC-A is reaching the default gateway on R1 g0/1.10, but the packet stops at the router.

1. You have already verified the routing table entries for R1, now execute the **show run | section interface** command to verify VLAN configuration. List any configuration errors.

\_\_int g0/1.1 jest przypisay do vlan 11 zamiast do vlan 1 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

What commands would resolve any issues found?

\_\_\_\_\_int g0/1.1 → encapsulation dot1Q 1 → intg0/1.10 → ip add 192.168.10.1 255.255.255.0 → end \_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Verify that that pings from PC-A now reach both S1 and S2.

From PC-A, is it possible to ping S1? \_\_\_\_tak\_\_\_

From PC-A, is it possible to ping S2? \_\_\_\_tak\_\_\_\_\_

1. Reflection

What are the advantages of viewing the routing table for troubleshooting purposes?

\_\_\_wszystkie interfejsy są wylistowane I mogą być w łatwy sposób sprawdzane gdzie został popełniony błąd \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Router Interface Summary Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Router Interface Summary | | | | |
| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| **Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface. | | | | |