
Lab – Troubleshooting IPv4 and IPv6 Static Routes

1. Topology



1. Addressing Table

|  |  |  |  |
| --- | --- | --- | --- |
| Device | Interface | IP Address | Default Gateway |
| HQ | G0/1 | 192.168.0.1/25  2001:DB8:ACAD::1/64  FE80::1 link-local | N/A |
|  | S0/0/0 (DCE) | 10.1.1.2/30  2001:DB8:ACAD:20::2/64 | N/A |
|  | S0/0/1 | 192.168.0.253/30  2001:DB8:ACAD:2::1/64 | N/A |
| ISP | G0/0 | 172.16.3.1/24  2001:DB8:ACAD:30::1/64  FE80::1 link-local | N/A |
|  | S0/0/0 | 10.1.1.1/30  2001:DB8:ACAD:20::1/64 | N/A |
| BRANCH | G0/1 | 192.168.1.1/24  2001:DB8:ACAD:1::1/64  FE80::1 link-local | N/A |
|  | S0/0/0 (DCE) | 192.168.0.254/30  2001:DB8:ACAD:2::2/64 | N/A |
| S1 | VLAN 1 | N/A | N/A |
| S3 | VLAN 1 | N/A | N/A |
| PC-A | NIC | 192.168.0.3/25  2001:DB8:ACAD::3/64 | 192.168.0.1  FE80::1 |
| Web Server | NIC | 172.16.3.3/24  2001:DB8:ACAD:30::3/64 | 172.16.3.1  FE80::1 |
| PC-C | NIC | 192.168.1.3/24  2001:DB8:ACAD:1::3/64 | 192.168.1.1  FE80::1 |

1. Objectives

Part 1: Build the Network and Configure Basic Device Settings

Part 2: Troubleshoot Static Routes in an IPv4 Network

Part 3: Troubleshoot Static Routes in an IPv6 Network

1. Background / Scenario

As a network administrator, you must be able to configure routing of traffic using static routes. Understanding how to configure and troubleshoot static routing is a requirement. Static routes are commonly used for stub networks and default routes. Your company’s ISP has hired you to troubleshoot connectivity issues on the network. You will have access to the HQ, BRANCH, and the ISP routers.

In this lab, you will begin by loading configuration scripts on each of the routers. These scripts contain errors that will prevent end-to-end communication across the network. You will need to troubleshoot each router to determine the configuration errors, and then use the appropriate commands to correct the configurations. When you have corrected all of the configuration errors, the hosts on the network should be able to communicate with each other.

**Note**: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.

**Note**: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.

1. Required Resources

* 3 Routers (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
* 2 Switches (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
* 3 PCs (Windows 7, Vista, or XP with terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet and serial cables as shown in the topology

1. Build the Network and Configure Basic Device Settings

In Part 1, you will set up the network topology and configure the routers and switches with some basic settings, such as passwords and IP addresses. Preset configurations are also provided for you for the initial router configurations. You will also configure the IP settings for the PCs in the topology.

* 1. Cable the network as shown in the topology.

Attach the devices as shown in the topology diagram and cable, as necessary.

* 1. Initialize and reload the routers and switches.
  2. Configure basic settings for each router.
     1. Disable DNS lookup.
     2. Configure device name as shown in the topology.
     3. Assign **class** as the privileged EXEC mode password.
     4. Assign **cisco** as the console and vty passwords.
     5. Configure **logging synchronous** to prevent console messages from interrupting command entry.
  3. Configure hosts and Web Server.
     1. Configure IP addresses for IPv4 and IPv6.
     2. Configure IPv4 default gateway.
  4. Load router configurations.

Router HQ

hostname HQ

ipv6 unicast-routing

interface GigabitEthernet0/1

ipv6 address 2001:DB8:ACAD::1/64

ip address 192.168.0.1 255.255.255.128

ipv6 address FE80::1 link-local

interface Serial0/0/0

ipv6 address 2001:DB8:ACAD:20::2/64

ip address 10.1.1.2 255.255.255.252

clock rate 800000

no shutdown

interface Serial0/0/1

ipv6 address 2001:DB8:ACAD:2::3/64

ip address 192.168.0.253 255.255.255.252

no shutdown

ip route 172.16.3.0 255.255.255.0 10.1.1.1

ip route 192.168.1.0 255.255.255.0 192.16.0.254

ipv6 route 2001:DB8:ACAD:1::/64 2001:DB8:ACAD:2::2

ipv6 route 2001:DB8:ACAD:30::/64 2001:DB8:ACAD::20:1

Router ISP

hostname ISP

ipv6 unicast-routing

interface GigabitEthernet0/0

ipv6 address 2001:DB8:ACAD:30::1/64

ip address 172.16.3.11 255.255.255.0

ipv6 address FE80::1 link-local

no shutdown

interface Serial0/0/0

ipv6 address 2001:DB8::ACAD:20:1/64

ip address 10.1.1.1 255.255.255.252

no shutdown

ip route 192.168.1.0 255.255.255.0 10.1.1.2

ipv6 route 2001:DB8:ACAD::/62 2001:DB8:ACAD:20::2

Router BRANCH

hostname BRANCH

ipv6 unicast-routing

interface GigabitEthernet0/1

ipv6 address 2001:DB8:ACAD:1::1/64

ip address 192.168.1.1 255.255.255.0

ipv6 address FE80::1 link-local

no shutdown

interface Serial0/0/0

ipv6 address 2001:DB8:ACAD:2::2/64

clock rate 128000

ip address 192.168.0.249 255.255.255.252

clock rate 128000

no shutdown

ip route 0.0.0.0 0.0.0.0 10.1.1.2

ipv6 route ::/0 2001:DB8:ACAD::1

1. Troubleshoot Static Routes in an IPv4 Network
2. IPv4 Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| HQ | G0/1 | 192.168.0.1 | 255.255.255.0 | N/A |
|  | S0/0/0 (DCE) | 10.1.1.2 | 255.255.255.252 | N/A |
|  | S0/0/1 | 192.168.0.253 | 255.255.255.252 | N/A |
| ISP | G0/0 | 172.16.3.1 | 255.255.255.0 | N/A |
|  | S0/0/0 | 10.1.1.1 | 255.255.255.252 | N/A |
| BRANCH | G0/1 | 192.168.1.1 | 255.255.255.0 | N/A |
|  | S0/0/0 (DCE) | 192.168.0.254 | 255.255.255.252 | N/A |
| S1 | VLAN 1 | 192.168.0.11 | 255.255.255.128 | 192.168.0.1 |
| S3 | VLAN 1 | 192.168.1.11 | 255.255.255.0 | 192.168.1.1 |
| PC-A | NIC | 192.168.0.3 | 255.255.255.128 | 192.168.0.1 |
| Web Server | NIC | 172.16.3.3 | 255.255.255.0 | 172.16.3.1 |
| PC-C | NIC | 192.168.1.3 | 255.255.255.0 | 192.168.1.1 |

* 1. Troubleshoot the HQ router.

The HQ router is the link between the ISP router and the BRANCH router. The ISP router represents the outside network while the BRANCH router represents the corporate network. The HQ router is configured with static routes to ISP and BRANCH networks.

* + 1. Display the status of the interfaces on HQ. Enter **show ip interface brief**. Record and resolve any issues as necessary.

\_\_\_\_int g0/1 jest shutdown, trzeba go zrobic no shut\_\_\_\_

* + 1. Ping from HQ router to BRANCH router (192.168.0.254). Were the pings successful? \_\_nie\_\_\_\_\_\_
    2. Ping from HQ router to ISP router (10.1.1.1). Were the pings successful? \_\_\_tak\_\_\_\_\_
    3. Ping from PC-A to the default gateway. Were the pings successful? \_\_\_\_\_tak\_\_\_
    4. Ping from PC-A to PC-C. Were the pings successful? \_\_\_nie\_\_\_\_\_
    5. Ping from PC-A to Web Server. Were the pings successful? \_\_nie\_\_\_\_\_\_
    6. Display the routing table on HQ. What non-directly connected routes are shown in the routing table?

\_\_\_statyczna ścieżka 172.16.3.0/24 przez 10.1.1.1, brak ścieżki do 192.168.1.0/24\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_\_sieć posiada statyczną ścieżkę do sieci pc-c ale nie pojawia się ona w tabeli, trzeba sprawić aby była ona poprawnie zkonfigurowana, jest też statyczna ścieżka do 172.16.3.0 ale web serwer jest nieosiągalny\_\_\_\_\_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

\_\_\_\_\_\_no ip route 192.168.1.0 255.255.255.0 192.16.0.254 → ip route 192.168.1.0 255.255.255.0 192.168.0.254\_\_\_\_\_\_\_\_\_

* + 1. Repeat any of the steps from b to f to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_\_\_router hq ciągle nie może pingować routera branch, sugeruje to że występują błędy na routerze branch które uniemożliwiają pc-a spingowanie pc-c, hq moze spingowac isp ale pca nie może spingować web serwer\_\_\_\_\_\_\_\_\_\_\_\_\_

* 1. Troubleshoot the ISP router.

For the ISP router, there should be a route to HQ and BRANCH routers. One static route is configured on ISP router to reach the 192.168.1.0/24, 192.168.0.0/25, and 192.168.0.252/30 networks.

* + 1. Display the status of interfaces on ISP. Enter **show ip interface brief**. Record and resolve any issues as necessary.

\_\_\_adres ip dla g0/0 jest niepoprawnie skonfigurowany\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Ping from the ISP router to the HQ router (10.1.1.2). Were the pings successful? \_\_\_\_tak\_\_\_\_
    2. Ping from Web Server to the default gateway. Were the pings successful? \_\_\_\_tak\_\_\_\_
    3. Ping from Web Server to PC-A. Were the pings successful? \_\_\_\_nie\_\_\_\_
    4. Ping from Web Server to PC-C. Were the pings successful? \_\_\_\_nie\_\_\_\_
    5. Display the routing table on ISP. What non-directly connected routes are shown in the routing table?

\_\_\_\_statyczna ścieżka do 192.168.1.0/24 przez 10.1.1.2, brak ście\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_potrzebna jest droga do 192.168.0.0/23 aby dojść do 192.168.1.0/24 I 192.168.0.252/30\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

(Hint: ISP only requires one summarized route to the company’s networks 192.168.1.0/24, 192.168.0.0/25, and 192.168.0.252/32.)

\_\_\_no ip route 192.168.1.0 255.255.255.0 10.1.1.2 → ip route 192.168.0.0 255.255.254.0 10.1.1.2\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Repeat any of the steps from b to e to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_teraz pca moze dojsc do web serwera lecz pcc nie, czyli cos dalej trzeba poprawic\_\_\_\_\_\_\_\_

* 1. Troubleshoot the BRANCH router.

For the BRANCH router, a default route is set to reach the rest of the network and ISP.

* + 1. Display the status of the interfaces on BRANCH. Enter **show ip interface brief**. Record and resolve any issues, as necessary.

\_\_\_\_s0/0/1 ma niepoprawny adres ip, int s0/0/0 → ip add 192.168.0.254 255.255.255.252\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Ping from the BRANCH router to the HQ router (192.168.0.253). Were the pings successful? \_tak\_\_\_\_
    2. Ping from PC-C to the default gateway. Were the pings successful? \_\_\_tak\_\_
    3. Ping from PC-C to PC-A. Were the pings successful? \_\_nie\_\_\_
    4. Ping from PC-C to Web Server. Were the pings successful? \_\_nie\_\_\_\_
    5. Display the routing table on BRANCH. What non-directly connected routes are shown in the routing table?

\_\_\_\_\_żadne\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_\_nie pokazują się statyczne ścieżki, domyślna ścieżka została niepoprawnie skonfigurowana \_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

\_\_\_no ip route 0.0.0.0 0.0.0.0 10.1.1.2 → ip route 0.0.0.0 0.0.0.0 192.168.0.253\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Repeat any of the steps from b to e to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_\_\_\_trzeba naprawić błędy w routerze hq\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Troubleshoot Static Routes in an IPv6 Network

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IPv6 Address | Prefix Length | Default Gateway |
| HQ | G0/1 | 2001:DB8:ACAD::1 | 64 | N/A |
|  | S0/0/0 (DCE) | 2001:DB8:ACAD::20:2 | 64 | N/A |
|  | S0/0/1 | 2001:DB8:ACAD:2::1 | 64 | N/A |
| ISP | G0/0 | 2001:DB8:ACAD:30::1 | 64 | N/A |
|  | S0/0/0 | 2001:DB8:ACAD:20::1 | 64 | N/A |
| BRANCH | G0/1 | 2001:DB8:ACAD:1::1 | 64 | N/A |
|  | S0/0/0 (DCE) | 2001:DB8:ACAD:2::2 | 64 | N/A |
| PC-A | NIC | 2001:DB8:ACAD::3 | 64 | FE80::1 |
| Web Server | NIC | 2001:DB8:ACAD:30::3 | 64 | FE80::1 |
| PC-C | NIC | 2001:DB8:ACAD:1::3 | 64 | FE80::1 |

* 1. Troubleshoot the HQ router.

The HQ router is the link between the ISP router and the BRANCH router. The ISP router represents the outside network while the BRANCH router represents the corporate network. The HQ router is configured with static routes to both the ISP and the BRANCH networks.

* + 1. Display the status of the interfaces on HQ. Enter **show ipv6 interface brief**. Record and resolve any issues, as necessary.

\_\_\_\_ipv6 interfejsu s0/0/1 jest niepoprawnie skonfigurowane \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Ping from the HQ router to the BRANCH router (2001:DB8:ACAD:2::2). Were the pings successful? \_tak\_
    2. Ping from the HQ router to the ISP router (2001:DB8:ACAD:20::1). Were the pings successful? \_\_\_nie\_
    3. Ping from PC-A to the default gateway. Were the pings successful? \_\_tak\_\_\_
    4. Ping from PC-A to Web Server. Were the pings successful? \_\_\_nie\_
    5. Ping from PC-A to PC-C. Were the pings successful? \_\_\_nie\_\_\_
    6. Display the routing table by issuing a **show ipv6 route** command. What non-directly connected routes are shown in the routing table?

\_\_\_\_2001:DB8:ACAD:1::/64 przez 2001:DB8:ACAD:2::2, 2001:DB8ACAD:30::/64 przez 2001:DB8:ACAD::20:1\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_\_statyczna ścieżka do 2001:DB8:ACAD:30::/64 ma niepoprawnie skonfigurowany następny adres skoku \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

\_\_\_\_no ipv6 route 2001:DB8:ACAD:30::/64 2001:DB8:ACAD::20:1 → ipv6 route 2001:db8:acad:30::/64 2001:db8:acad:20::1 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Repeat any of the steps from b to f to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_\_\_problemy routingu nie zostały rozwiązane, problem musi znajdować się w isp\_\_\_\_\_\_\_\_\_\_\_\_

* 1. Troubleshoot the ISP router.

On the ISP router, one static route is configured to reach all the networks on HQ and BRANCH routers.

* + 1. Display the status of the interfaces on ISP. Enter **show ipv6 interface brief**. Record and resolve any issues, as necessary.

\_\_\_adres ipv6 w interfejsie s0/0/0 jest niepoprawnie skonfigurowany\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Ping from the ISP router to the HQ router (2001:DB8:ACAD:20::2). Were the pings successful? \_\_tak\_\_
    2. Ping from Web Server to the default gateway. Were the pings successful? \_\_\_\_\_tak\_\_\_
    3. Ping from Web Server to PC-A. Were the pings successful? \_\_\_\_\_tak\_\_\_
    4. Ping from Web Server to PC-C. Were the pings successful? \_\_\_\_nie\_\_\_\_
    5. Display the routing table. What non-directly connected routes are shown in the routing table?

\_\_\_\_\_\_2001:db8:acad::/62\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_\_\_nie ma porblemów z statyczną ścieżką \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

\_\_\_\_nie trzeba rozwiązywać problemów \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Repeat any of the steps from b to e to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_\_\_\_\_\_pc-c ciągle nie może pingować web server\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* 1. Troubleshoot the BRANCH router.

For the BRANCH routers, there is a default route to the HQ router. This default route allows the BRANCH network to the ISP router and Web Server.

* + 1. Display the status of the interfaces on BRANCH. Enter **show ipv6 interface brief**. Record and resolve any issues, as necessary.

\_\_\_\_Według tabeli wszystkie zostały skonfigurowane poprawnie\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Ping from the BRANCH router to the HQ router (2001:DB8:ACAD:2::1). Were the pings successful? \_\_\_\_\_\_tak\_\_
    2. Ping from the BRANCH router to the ISP router (2001:DB8:ACAD:20::1). Were the pings successful? \_\_\_\_\_\_nie\_\_
    3. Ping from PC-C to the default gateway. Were the pings successful? \_\_\_\_\_tak\_\_\_
    4. Ping from PC-C to PC-A. Were the pings successful? \_\_nie\_\_\_\_\_\_
    5. Ping from PC-C to Web Server. Were the pings successful? \_\_\_\_nie\_\_\_\_
    6. Display the routing table. What non-directly connected routes are shown in the routing table?

\_\_\_\_\_\_żadne\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Based on the results of the pings, routing table output, and static routes in the running configuration, what can you conclude about network connectivity?

\_\_\_\_\_\_\_nie ma domyślnej ściezki, adres następnego skoku jest niepoprawnie skonfigurowany \_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. What commands (if any) need to be entered to resolve routing issues? Record the command(s).

\_\_\_\_no ipv6 route ::/0 2001:db8:acad::1 → ipv6 route ::/0 2001:db8:acad:2::1 \_\_\_

* + 1. Repeat any of the steps from b to f to verify whether the problems have been resolved. Record your observations and possible next steps in troubleshooting connectivity.

\_\_\_\_teraz problemy zostały rozwiązane, mozemy pingowac web server I pcc z pca \_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Router Interface Summary Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Router Interface Summary | | | | |
| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| **Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface. | | | | |